How to run the simulation ?

1. Without disturbance: One needs to open the init.m file and run the script.

2. With disturbance: Open the Simulink model file named “quad\_control” and then open the subsystem named “model”. In the model subsystem one can see the step disturbance block . Edit the parameters of the step disturbance block as per requirement.